EXTERNAL PORTS
These are the external ports defined in the MHS file.
Attributes Key The attributes are obtained from the SIGIS and IOB_STATE parameters set on the PORT in the MHS file CLK indicates Clock ports, (SIGIS = CLK) INTR indicates Interrupt ports,(SIGIS = INTR) RESET indicates Reset ports, (SIGIS = RST) BUF or REG Indicates ports that instantiate or infer IOB primitives, (IOB_STATE = BUF or REG)
# | NAME | DIR | [LSB:MSB] | SIG | ATTRIBUTES